**?.?? PSS Chilled Water Buffer Vessel**

The Mechanical Contractor shall supply and install a Chilled Water Vessel, as supplied by Commercial Hot Water Solutions Ltd (contact Richard Bailey, email: richard@chwsltd.co.uk tel: 07530 230 838) from their PSS range, in accordance with the following schedule:-

* Model ref: PSS
* Vessel Capacity: 200 litres

The PSS Chilled Water Vessel shall strictly comprise the following features: high quality steel construction, 50mm soft polyurethane insulation with anti-condensation protection, maximum working temperature of 95 Deg C.