**?.?? Indirect Domestic Hot Water Cylinder / Calorifier**

The Mechanical Contractor shall supply and install an indirect domestic hot water cylinder / calorifier as supplied by Commercial Hot Water Solutions Ltd (contact Richard Bailey, email: richard@chwsltd.co.uk tel: 07530 230 838) from their ProStor XS range, in accordance with the following schedule:

* Model ref: ProStor XS 1000
* Vessel Capacity: 919 litres
* Coil Surface Area: 3.57 m2
* Coil Output: 112 kw

The cylinder shall strictly comprise the following features; suitable for domestic hot water generation, stainless steel construction, fixed single coil, 100mm Soft Polyurethane Insulation Jacket, 6 bar working pressure, 100 Deg C maximum working temperature, inspection hatch, destratification tappings, electrical immersion port and 3x ½” sensor tappings.